**ALVIC Checklist**

*MUST complete one form for each quote*

* Dealer Name:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_
* Dealer ID#:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_
* Designer contact:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_
* Designer phone#:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_
* Email:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_
* Alvic Series : Syncron Luxe Zenit (select one)
* Grain direction: Horizontal Vertical No-Grain (select one)
* Color: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_
* Edge Banding: Add $274 charge per color
* Please submit the 2020 or ProKitchen floorplan drawings in PDF, NOT jpeg

**IMPORTANT details specific to ALVIC:**

**FINISHED ENDS = APPLIED PANELS**

* Allow ¾” for APPLIED end panels / finished ends
  + Base/Tall End Panel = 25” depth
  + Wall End Panel = 13” depth
* All panels are to be applied in the field

**FRIDGE & DISHWASHER PANELS**

* REP and DWR come with front 3” stile/filler as a separate piece, to be installed in the field.

**GRAIN DIRECTION**

* VERTICAL GRAIN is the default
* HORTIZONTAL GRAIN maximum panel height = 47”